|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Checked by Supervisor / Initials & date** | | | |  | | | | | | | |
| **Location:** | | | | **SAM Details:** | | | | | | | |
|
| **Company Name:** | | | | **Date:**  **Start time: Finish Time:** | | | | | | | |
|
| **Staff name:** | | | | **Staff name:** | | | | | | | |
|
| **Team Leader (Print):** | | | | **Signature:** | | | | | | | |
| Daily Completion | | | | | | | | | | | |
| Heat Shrink In Line Joint / Address | Work comp |  | | | | |  | | | | |
| Location From |  | | | | Location To | |  | | |
|  | |  | |  | |  |
|  |  |  |  | |  | |  | |  | |  |
|  |  |  |  | |  | |  | |  | |  |
|  |  |  |  | |  | |  | |  | |  |
| **IN PROCESS INSPECTION FOR IN LINE JOINTS** | | | | | | **Y** | | **N** | | **N/A** | |
| Correct type & size of joint closure. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Correct number & size of cables in main port / auxiliary port | | | | | | 🞎 | | 🞎 | | 🞎 | |
| SCOP’s installed on PE sheathed cable. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Aluminium foil applied to MB & PE sheathed cables | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Linen tape applied to MB cable sheath | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Branch joints fitted with correct Branch clip between each additional cable. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Number of cables inserted in end of In Line Joint does not exceed 4. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Correct positioning of Hard Jacket. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Correct position of Sheath inside Joint. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Approved connectors used & pairs jointed correctly. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Two white lines visible under closure channel. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Adequate show of adhesive around end of sleeve. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Adequate mix of the adhesive colours in the area of the branch clip. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Physical recovery of the sleeve conforms to the general shape of the internal canister & cables. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Thermochromic paint on sleeve has changed colour completely. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Moisture barrier screens of MB sheathed cables are electrically continuous. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Tie cables from Pillar to node labelled in Pit or Manhole. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Cables labelled to standard at Joint. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Correct cable layout & length left in Pit or Manhole. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Joint supported. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Joint not installed in EPR zone | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Site left safe. | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
| **Comments:** | | | | | | | | | | | |