|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Checked by Supervisor / Initials & date** | | | |  | | | | | | | |
| **Location:** | | | | **SAM Details:** | | | | | | | |
|
| **Company Name:** | | | | **Date:**  **Start time: Finish Time:** | | | | | | | |
|
| **Staff name:** | | | | **Staff name:** | | | | | | | |
|
| **Team Leader (Print):** | | | | **Signature:** | | | | | | | |
| Daily Completion | | | | | | | | | | | |
| PVC Joint / Address | Work comp |  | | | | |  | | | | |
| Location From |  | | | | Location To | |  | | |
|  | |  | |  | |  |
|  |  |  |  | |  | |  | |  | |  |
|  |  |  |  | |  | |  | |  | |  |
|  |  |  |  | |  | |  | |  | |  |
| **IN PROCESS INSPECTION FOR PVC JOINT** | | | | | | **Y** | | **N** | | **N/A** | |
| Filled cable sheath extended about 30mm above apoxy. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Epoxy resin present in ports containing air cored plastic cable. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Unit whippings removed from air cored cable. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Butyl rubber and PVC tape used to seal joint. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Shroud installed. PVC S & L joint only. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| PVC cover installed to standard. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Epoxy resin used to seal port. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Pair / Unit collets used | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Mesh unit bags fitted to standard. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Conductor length to standard on new work. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Approved connectors used / pairs jointed correctly & obsolete connectors have been replaced. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Correct connector selection used to reduce customer disruption. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Have any Faulty connectors not been replaced. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Encapsulant gel removed to top of base where required in existing joints. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Conductor insulation not damaged when gel has been removed. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Cables labelled to standard at joints. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Lead-in labelled at Distribution Joint | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Support Bar / bracket fitted / not too short. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Correct cable layout in pit or manhole & Sufficient cable length left in pit. | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Joint supported | | | | | | 🞎 | | 🞎 | | 🞎 | |
| Site left safe. | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
|  | | | | | | 🞎 | | 🞎 | | 🞎 | |
| **Comments:** | | | | | | | | | | | |