|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Checked by Supervisor / Initials & date** | | | |  | | | | |
| **Location:** | | | | **SAM Details:** | | | | |
|
| **Company Name:** | | | | **Date:**  **Start time: Finish Time:** | | | | |
|
| **Staff name:** | | | | **Staff name:** | | | | |
|
| **Team Leader (Print):** | | | | **Signature:** | | | | |
| Daily Completion | | | | | | | | |
| Fibre Testing / Address |  |  |  | |  |  |  |  |
| Work comp |  |  | |  |  |  |  |
|  |  |  |  | |  |  |  |  |
|  |  |  |  | |  |  |  |  |
|  |  |  |  | |  |  |  |  |
|  |  |  |  | |  |  |  |  |
|  |  |  |  | |  |  |  |  |
| **IN PROCESS INSPECTION FOR OPTICAL FIBRE TESTING** | | | | | | **Y** | **N** | **N/A** |
| Correct fibre hygiene practices utilised. No connector end face contamination or damage. | | | | | | 🞎 | 🞎 | 🞎 |
| Link loss readings are within acceptable range. | | | | | | 🞎 | 🞎 | 🞎 |
| No single event loss exceeds criteria. | | | | | | 🞎 | 🞎 | 🞎 |
| SOR trace file number aligns to Spatial records. | | | | | | 🞎 | 🞎 | 🞎 |
| Correct connectivity in accordance with spatial/splice records. | | | | | | 🞎 | 🞎 | 🞎 |
| Has OTDR pulse width been set for cable distance? | | | | | | 🞎 | 🞎 | 🞎 |
| Has a minimum of 150m launch spool been used & distance subtracted from the link under test for optical budget calculations. | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
|  | | | | | | 🞎 | 🞎 | 🞎 |
| Splicer Used? Model: Serial no: Service Date  Cleaver Used? Model: Serial no: Service Date | | | | | | 🞎 | 🞎 | 🞎 |
| **Comments:** | | | | | | | | |